


مشخصات فنی

|  |  |  |
| --- | --- | --- |
| **Phone Features** | **Codes and Voice Features** | **Physical Features** |
| 2, 4, 8 SIP accounts, Hotline | Wideband Codec: G.722 | 320x80 graphic LCD |
| Call hold, waiting, forward, return | Narrowband codec: G.711μ/A, G.723.1 | 45 keys, including 20 programmable keys |
| Call transfer (blind/busy/ask) | G.726, G.729AB, iLBC | Wall-mountable |
| Caller ID display, Redial, Mute, DND | VAD, CNG, AEC, AGC, Full-duplex | 1\* RJ-9 handset port |
| Auto-answer, 3-way conferencing |  | 1\*RJ-9 headset port |
| Speed dial, SMS, Voicemail | **Security** | 1\*3.5mm PC headset port |
| Message Waiting Indication LED | VLAN QoS (802.1p, 802.1q) | 2xRJ45 10/100/1000M Ethernet ports |
| Tone scheme, Volume control | Phone lock for personal privacy protection | Direct Power and POE |
| Direct IP call without a server | Admin/User 2-level configuration mode, LLDP, CDP | Power consumption: 2.5-3.5W |
| Ring tone selection/import/delete | L2TP VPN , SRTP, TLS | Operating humidity: up to 95% |
| Black list, Hand-free indicator. |  | Storage temperature: up to 60°C |
| Call history: dialed/received/missed | **Network Features** |  |
| Programmable Soft key | SIP v1 (RFC2543), v2 (RFC3261) | **Compliance** |
| Supports PC control | SIP connection: Proxy mode & Peering Points mode | Ericsson  Alcatel  Huawei  ZTE  NEC  Mitel  Avaya  Asterisk  Freeswitch  3CX |
| **Advanced Features** | DNS SRV (RFC3263)  Redundant server support |  |
| XML Phone Book search and input & output  Enterprise phone book(800 entries) | NAT Traversal: STUN mode  DTMF: In-Band, RFC2833, SIP Info, Auto |  |
| LDAP phone book | Web Management (HTTP, HTTPS) |  |
| Functions customizable keys | IP Assignment: Static, DHCP, PPPoE |  |
| Support up to 20 programmable keys | Transparent Bridge, Router PC Port |  |
|  | TFTP, DHCP, PPPoE client |  |
| **IP PBX System Integration** | DNS client, NAT, DHCP server |  |
| Busy lamp field (BLF), BLF list | Layer 3 ToS, DSCP |  |
| Bridged line appearance (BLA) |  |  |
| DND & Forward synchronization | **Management** |  |
| Intercom, Paging, Music on hold | Auto-provision via FTP, TFTP, HTTP, HTTPS |  |
| Call pickup, Dial Plan, Call recording | Configuration: browser, phone, auto-provision |  |
| Anonymous call rejection | Trace package and system log export |  |
| Network conference, Distinctive ringtone |  |  |



www.raytronik.ir

info@raytronik.ir

کارخانه: کرج، شهرک صنعتی بهارستان، گلستان 6، تاکستان، پلاک 2

تلفن 44716393، فکس: 44716404

دفتر مرکزی: تهران، شهرک گلستان، خیابان گلها، خیابان یاسمن، پلاک 2